These scripts will load (load_sw) and plot (plot_sw) water saturation distribution (keyword OUTPUT item 2) in 2D. The network is assumed to be a random 3D network. All elements within a section of the network will be plotted in 2D.